Bus Passenger Shelter Professional Specification & Materials

**STAINLESS STEEL FRAMING**

High resistance against rust/ corrosion **& FIXINGS** no painting or re-painting required Quality appearance Long life - Low maintenance Concealed edges for glazing.

**FLAT ROOF**

Low maintenance with coloured infill or translucent panelling to roof section

**BARRELLED ROOF SECTION**

Barrelled - clear /translucent glazing & stainless steel framing with GRP end panels (Colour choice)

**GLAZING**

UV Inhibited 4 mm polycarbonate/ (5 and 6 mm, tinted avail. at extra cost) **Toughened glass available 4 & 6 mm.** Various infill panels, in various colours & thicknesses depending on site YOUR COAT OF ARMS etched/coloured vinyl

**INFILL PANELS**

Coloured infill - Lower infill and full panels available Mitglass:built in colour rust proof & can be cleaned Patterned steel for 'no-go areas'

**LOGO PANELS** Coloured logo panels, with lettering e.g. Council name/logo/route included Colour choice to match roof ends

**SEATING AVAILABLE**

Stainless steel perch type seating dimensions depend on shelter configuration

**COLOUR CHOICE** logo/name boards /end caps/ roof top

**TIME TABLE**

**FITTING/INSTALLATION** Fitting team available

VARIOUS LENGTHS OF SHELTERS AVAIL 2.0M, 2.5M, 3.0M, 3.5M and upwards

WINDBREAK-ENDS 300 MM UP TO 1.0M